Board:

Button: Start transmission or not

LED: Indicating the transmission

Arduino:

Adaptive Threshold

GUI:

Signal Processing: FFT, adaptive threshold, Low pass filter, auto selecting heart rate

Save Function

Heart rate warning selection

Transmission unstable detection

Pulse zoom in